Westermo Bench Power Cable

The intent of this cable is to power a Westermo switch on the bench to set the programming or to check functionality.

Parts

1. M12 female B coded 4 position plug digikey pn A1333878-ND
2. 2-4 ft wire 16GA minimum
3. 1 red trimet banana clip
4. 1 black trimet banana clip

Assembly

1. Grab one wire and attach the red banana clip
2. Hook up the wire with the red banana clip to terminal 1
3. Grab the remaining wire and attach the black banana clip
4. Hook up the wire with the black banana clip to terminal 3

